Before & After Airflow Report
Record comparable measurements and the work completed. Leave a copy with the customer.
	Customer
	[CUSTOMER NAME]

	Service address
	[SERVICE ADDRESS]

	Service date
	[DATE]

	Technician
	[TECHNICIAN NAME]



Measurement conditions
Keep these the same every time, so this year's reading can be compared to next year's.
	Measured at
	☐ Exterior vent cap ☐ Dryer outlet ☐ Other: ______

	Instrument & units
	[ANEMOMETER MODEL] · ☐ m/s ☐ ft/min

	Dryer setting
	☐ Air-only / no heat ☐ Other: ______

	Vent exits through
	☐ Side wall ☐ Roof ☐ Other: ______



Readings
	Measurement
	Before
	After

	Airflow reading
	
	

	Time measured
	
	

	Lint trap clean at start?
	☐ Yes ☐ No
	—



Work completed
☐ Disconnected and reconnected the dryer
☐ Brushed and vacuumed the reachable duct
☐ Cleaned the exterior vent cap
☐ Checked the exterior flap opens freely
☐ Other: ______
What we found


Recommendations
☐ Next cleaning: [MONTH / YEAR]
☐ Replace transition duct behind the dryer
☐ Other: ______

Compare readings only when they were taken with the same instrument, units, location and dryer setting. An airflow reading on its own does not certify a dryer or vent as safe.
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